From 82fa50eadf11f01e6315f5e2c2a29845e2a516b8 Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Mon, 8 Apr 2019 03:49:26 +0200
Subject: [PATCH] Fix reset issue on H6 by using R_WDOG

Inspired by froezuses patch here:

https://forum.armbian.com/topic/9833-h6-famous-reboot-problem/?page=3

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 plat/allwinner/sun50i_h6/include/sunxi_mmap.h | 3 +++
 1 file changed, 3 insertions(+)

diff --git a/plat/allwinner/sun50i_h6/include/sunxi_mmap.h b/plat/allwinner/sun50i_h6/include/sunxi_mmap.h
index f36491a8..f01745a4 100644
--- a/plat/allwinner/sun50i_h6/include/sunxi_mmap.h
+++ b/plat/allwinner/sun50i_h6/include/sunxi_mmap.h
@@ -58,4 +58,7 @@
 #define SUNXI_R_UART_BASE		0x07080000
 #define SUNXI_R_PIO_BASE		0x07022000
 
+#undef SUNXI_WDOG_BASE
+#define SUNXI_WDOG_BASE			SUNXI_R_WDOG_BASE
+
 #endif /* SUNXI_MMAP_H */
-- 
2.21.0
