From ab35c98369d50766eb20920a93a2dca927935481 Mon Sep 17 00:00:00 2001
From: OpenEmbedded <oe.patch@oe>
Date: Fri, 19 May 2023 23:01:14 +0200
Subject: [PATCH] Add usb support to h616. This is not needed from kernel 6.2

Signed-off-by: OpenEmbedded <oe.patch@oe>
---
 .../arm64/boot/dts/allwinner/sun50i-h616.dtsi | 160 ++++++++++++++++++
 1 file changed, 160 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
index 04cdec7e2..a1d872e74 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
@@ -504,6 +504,166 @@ mdio0: mdio {
 			};
 		};
 
+		usbotg: usb@5100000 {
+			compatible = "allwinner,sun50i-h616-musb",
+				     "allwinner,sun8i-h3-musb";
+			reg = <0x05100000 0x0400>;
+			clocks = <&ccu CLK_BUS_OTG>;
+			resets = <&ccu RST_BUS_OTG>;
+			interrupts = <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "mc";
+			phys = <&usbphy 0>;
+			phy-names = "usb";
+			extcon = <&usbphy 0>;
+			status = "disabled";
+		};
+
+		usbphy: phy@5100400 {
+			compatible = "allwinner,sun50i-h616-usb-phy";
+			reg = <0x05100400 0x24>,
+			      <0x05101800 0x14>,
+			      <0x05200800 0x14>,
+			      <0x05310800 0x14>,
+			      <0x05311800 0x14>;
+			reg-names = "phy_ctrl",
+				    "pmu0",
+				    "pmu1",
+				    "pmu2",
+				    "pmu3";
+			clocks = <&ccu CLK_USB_PHY0>,
+				 <&ccu CLK_USB_PHY1>,
+				 <&ccu CLK_USB_PHY2>,
+				 <&ccu CLK_USB_PHY3>,
+				 <&ccu CLK_BUS_EHCI2>;
+			clock-names = "usb0_phy",
+				      "usb1_phy",
+				      "usb2_phy",
+				      "usb3_phy",
+				      "pmu2_clk";
+			resets = <&ccu RST_USB_PHY0>,
+				 <&ccu RST_USB_PHY1>,
+				 <&ccu RST_USB_PHY2>,
+				 <&ccu RST_USB_PHY3>;
+			reset-names = "usb0_reset",
+				      "usb1_reset",
+				      "usb2_reset",
+				      "usb3_reset";
+			status = "disabled";
+			#phy-cells = <1>;
+		};
+
+		ehci0: usb@5101000 {
+			compatible = "allwinner,sun50i-h616-ehci",
+				     "generic-ehci";
+			reg = <0x05101000 0x100>;
+			interrupts = <GIC_SPI 26 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI0>,
+				 <&ccu CLK_BUS_EHCI0>,
+				 <&ccu CLK_USB_OHCI0>;
+			resets = <&ccu RST_BUS_OHCI0>,
+				 <&ccu RST_BUS_EHCI0>;
+			phys = <&usbphy 0>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
+		ohci0: usb@5101400 {
+			compatible = "allwinner,sun50i-h616-ohci",
+				     "generic-ohci";
+			reg = <0x05101400 0x100>;
+			interrupts = <GIC_SPI 27 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI0>,
+				 <&ccu CLK_USB_OHCI0>;
+			resets = <&ccu RST_BUS_OHCI0>;
+			phys = <&usbphy 0>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
+		ehci1: usb@5200000 {
+			compatible = "allwinner,sun50i-h616-ehci",
+				     "generic-ehci";
+			reg = <0x05200000 0x100>;
+			interrupts = <GIC_SPI 28 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI1>,
+				 <&ccu CLK_BUS_EHCI1>,
+				 <&ccu CLK_USB_OHCI1>;
+			resets = <&ccu RST_BUS_OHCI1>,
+				 <&ccu RST_BUS_EHCI1>;
+			phys = <&usbphy 1>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
+		ohci1: usb@5200400 {
+			compatible = "allwinner,sun50i-h616-ohci",
+				     "generic-ohci";
+			reg = <0x05200400 0x100>;
+			interrupts = <GIC_SPI 29 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI1>,
+				 <&ccu CLK_USB_OHCI1>;
+			resets = <&ccu RST_BUS_OHCI1>;
+			phys = <&usbphy 1>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
+		ehci2: usb@5310000 {
+			compatible = "allwinner,sun50i-h616-ehci",
+				     "generic-ehci";
+			reg = <0x05310000 0x100>;
+			interrupts = <GIC_SPI 30 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI2>,
+				 <&ccu CLK_BUS_EHCI2>,
+				 <&ccu CLK_USB_OHCI2>;
+			resets = <&ccu RST_BUS_OHCI2>,
+				 <&ccu RST_BUS_EHCI2>;
+			phys = <&usbphy 2>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
+		ohci2: usb@5310400 {
+			compatible = "allwinner,sun50i-h616-ohci",
+				     "generic-ohci";
+			reg = <0x05310400 0x100>;
+			interrupts = <GIC_SPI 31 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI2>,
+				 <&ccu CLK_USB_OHCI2>;
+			resets = <&ccu RST_BUS_OHCI2>;
+			phys = <&usbphy 2>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
+		ehci3: usb@5311000 {
+			compatible = "allwinner,sun50i-h616-ehci",
+				     "generic-ehci";
+			reg = <0x05311000 0x100>;
+			interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI3>,
+				 <&ccu CLK_BUS_EHCI3>,
+				 <&ccu CLK_USB_OHCI3>;
+			resets = <&ccu RST_BUS_OHCI3>,
+				 <&ccu RST_BUS_EHCI3>;
+			phys = <&usbphy 3>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
+		ohci3: usb@5311400 {
+			compatible = "allwinner,sun50i-h616-ohci",
+				     "generic-ohci";
+			reg = <0x05311400 0x100>;
+			interrupts = <GIC_SPI 33 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI3>,
+				 <&ccu CLK_USB_OHCI3>;
+			resets = <&ccu RST_BUS_OHCI3>;
+			phys = <&usbphy 3>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
 		rtc: rtc@7000000 {
 			compatible = "allwinner,sun50i-h616-rtc";
 			reg = <0x07000000 0x400>;
-- 
2.40.1

