From 767a05572ef5b93c2e157749b1754cbe261ee43d Mon Sep 17 00:00:00 2001
From: Marek Belisko <marek.belisko@open-nandra.com>
Date: Fri, 8 Apr 2022 11:33:53 +0200
Subject: [PATCH] Added nanopi-r1 board support

Patch taken from : https://github.com/armbian/build/blob/master/patch/u-boot/u-boot-sunxi/add-nanopi-r1-and-duo2.patch

Signed-off-by: Marek Belisko <marek.belisko@open-nandra.com>
---
diff --git a/configs/nanopi_r1_defconfig b/configs/nanopi_r1_defconfig
new file mode 100644
index 0000000..e028b41
--- /dev/null
+++ b/configs/nanopi_r1_defconfig
@@ -0,0 +1,22 @@
+CONFIG_ARM=y
+CONFIG_ARCH_SUNXI=y
+CONFIG_SPL=y
+CONFIG_MACH_SUN8I_H3=y
+CONFIG_DRAM_CLK=408
+CONFIG_DRAM_ZQ=3881979
+CONFIG_DRAM_ODT_EN=y
+CONFIG_MACPWR="PD6"
+# CONFIG_VIDEO_DE2 is not set
+CONFIG_NR_DRAM_BANKS=1
+# CONFIG_SYS_MALLOC_CLEAR_ON_INIT is not set
+CONFIG_CONSOLE_MUX=y
+CONFIG_SYS_CLK_FREQ=480000000
+# CONFIG_CMD_FLASH is not set
+# CONFIG_SPL_DOS_PARTITION is not set
+# CONFIG_SPL_EFI_PARTITION is not set
+CONFIG_DEFAULT_DEVICE_TREE="sun8i-h3-nanopi-r1"
+CONFIG_SUN8I_EMAC=y
+CONFIG_USB_EHCI_HCD=y
+CONFIG_USB_OHCI_HCD=y
+CONFIG_SYS_USB_EVENT_POLL_VIA_INT_QUEUE=y
+CONFIG_MMC_SUNXI_SLOT_EXTRA=2
-- 
2.7.4

