From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Kali Prasad <kprasadvnsi@protonmail.com>
Date: Sun, 19 Sep 2021 08:02:27 +0000
Subject: drv:nvmem:sunxi_sid: Support SID on H616

Add support for H616's SID controller. It supports 4K-bit
EFUSE.

Signed-off-by: Kali Prasad <kprasadvnsi@protonmail.com>
---
 drivers/nvmem/sunxi_sid.c | 7 +++++++
 1 file changed, 7 insertions(+)

diff --git a/drivers/nvmem/sunxi_sid.c b/drivers/nvmem/sunxi_sid.c
index 5d364d85347f..c526fe4abe22 100644
--- a/drivers/nvmem/sunxi_sid.c
+++ b/drivers/nvmem/sunxi_sid.c
@@ -204,6 +204,12 @@ static const struct sunxi_sid_cfg sun50i_h6_cfg = {
 	.size = 0x200,
 };
 
+static const struct sunxi_sid_cfg sun50i_h616_cfg = {
+	.value_offset = 0x200,
+	.size = 0x100,
+	.need_register_readout = true,
+};
+
 static const struct of_device_id sunxi_sid_of_match[] = {
 	{ .compatible = "allwinner,sun4i-a10-sid", .data = &sun4i_a10_cfg },
 	{ .compatible = "allwinner,sun7i-a20-sid", .data = &sun7i_a20_cfg },
@@ -213,6 +219,7 @@ static const struct of_device_id sunxi_sid_of_match[] = {
 	{ .compatible = "allwinner,sun50i-a64-sid", .data = &sun50i_a64_cfg },
 	{ .compatible = "allwinner,sun50i-h5-sid", .data = &sun50i_a64_cfg },
 	{ .compatible = "allwinner,sun50i-h6-sid", .data = &sun50i_h6_cfg },
+	{ .compatible = "allwinner,sun50i-h616-sid", .data = &sun50i_h616_cfg },
 	{/* sentinel */},
 };
 MODULE_DEVICE_TABLE(of, sunxi_sid_of_match);
-- 
Armbian

