From 83b0b8a7b9cb658d3cc980b4fbcbb2cc8b257ccf Mon Sep 17 00:00:00 2001
From: Trevor Woerner <twoerner@gmail.com>
Date: Thu, 24 Sep 2015 17:07:26 -0400
Subject: [PATCH] gcc5 fixes

gcc5 is pickier about inline functions defined in headers.

Signed-off-by: Trevor Woerner <twoerner@gmail.com>
---
 drivers/net/wireless/rtl8188eu/include/ieee80211.h | 4 ++--
 drivers/net/wireless/rtl8189es/include/ieee80211.h | 4 ++--
 drivers/net/wireless/rtl8192cu/include/ieee80211.h | 8 ++++----
 drivers/net/wireless/rtl8723as/include/ieee80211.h | 4 ++--
 drivers/staging/rtl8712/ieee80211.h                | 4 ++--
 5 files changed, 12 insertions(+), 12 deletions(-)

diff --git a/drivers/net/wireless/rtl8188eu/include/ieee80211.h b/drivers/net/wireless/rtl8188eu/include/ieee80211.h
index 1ae96a5..7a301c5 100644
--- a/drivers/net/wireless/rtl8188eu/include/ieee80211.h
+++ b/drivers/net/wireless/rtl8188eu/include/ieee80211.h
@@ -1188,12 +1188,12 @@ enum ieee80211_state {
 (((Addr[2]) & 0xff) == 0xff) && (((Addr[3]) & 0xff) == 0xff) && (((Addr[4]) & 0xff) == 0xff) && \
 (((Addr[5]) & 0xff) == 0xff))
 #else
-extern __inline int is_multicast_mac_addr(const u8 *addr)
+static __inline int is_multicast_mac_addr(const u8 *addr)
 {
         return ((addr[0] != 0xff) && (0x01 & addr[0]));
 }
 
-extern __inline int is_broadcast_mac_addr(const u8 *addr)
+static __inline int is_broadcast_mac_addr(const u8 *addr)
 {
 	return ((addr[0] == 0xff) && (addr[1] == 0xff) && (addr[2] == 0xff) &&   \
 		(addr[3] == 0xff) && (addr[4] == 0xff) && (addr[5] == 0xff));
diff --git a/drivers/net/wireless/rtl8189es/include/ieee80211.h b/drivers/net/wireless/rtl8189es/include/ieee80211.h
index 1ae96a5..7a301c5 100644
--- a/drivers/net/wireless/rtl8189es/include/ieee80211.h
+++ b/drivers/net/wireless/rtl8189es/include/ieee80211.h
@@ -1188,12 +1188,12 @@ enum ieee80211_state {
 (((Addr[2]) & 0xff) == 0xff) && (((Addr[3]) & 0xff) == 0xff) && (((Addr[4]) & 0xff) == 0xff) && \
 (((Addr[5]) & 0xff) == 0xff))
 #else
-extern __inline int is_multicast_mac_addr(const u8 *addr)
+static __inline int is_multicast_mac_addr(const u8 *addr)
 {
         return ((addr[0] != 0xff) && (0x01 & addr[0]));
 }
 
-extern __inline int is_broadcast_mac_addr(const u8 *addr)
+static __inline int is_broadcast_mac_addr(const u8 *addr)
 {
 	return ((addr[0] == 0xff) && (addr[1] == 0xff) && (addr[2] == 0xff) &&   \
 		(addr[3] == 0xff) && (addr[4] == 0xff) && (addr[5] == 0xff));
diff --git a/drivers/net/wireless/rtl8192cu/include/ieee80211.h b/drivers/net/wireless/rtl8192cu/include/ieee80211.h
index 86e9726..950691d 100644
--- a/drivers/net/wireless/rtl8192cu/include/ieee80211.h
+++ b/drivers/net/wireless/rtl8192cu/include/ieee80211.h
@@ -1149,12 +1149,12 @@ enum ieee80211_state {
 #define MAC_FMT "%02x:%02x:%02x:%02x:%02x:%02x"
 #define MAC_ARG(x) ((u8*)(x))[0],((u8*)(x))[1],((u8*)(x))[2],((u8*)(x))[3],((u8*)(x))[4],((u8*)(x))[5]
 
-extern __inline int is_multicast_mac_addr(const u8 *addr)
+static __inline int is_multicast_mac_addr(const u8 *addr)
 {
         return ((addr[0] != 0xff) && (0x01 & addr[0]));
 }
 
-extern __inline int is_broadcast_mac_addr(const u8 *addr)
+static __inline int is_broadcast_mac_addr(const u8 *addr)
 {
 	return ((addr[0] == 0xff) && (addr[1] == 0xff) && (addr[2] == 0xff) &&   \
 		(addr[3] == 0xff) && (addr[4] == 0xff) && (addr[5] == 0xff));
@@ -1177,7 +1177,7 @@ typedef struct tx_pending_t{
 #define IEEE_G            (1<<2)
 #define IEEE_MODE_MASK    (IEEE_A|IEEE_B|IEEE_G)
 
-extern __inline int ieee80211_is_empty_essid(const char *essid, int essid_len)
+static __inline int ieee80211_is_empty_essid(const char *essid, int essid_len)
 {
 	/* Single white space is for Linksys APs */
 	if (essid_len == 1 && essid[0] == ' ')
@@ -1193,7 +1193,7 @@ extern __inline int ieee80211_is_empty_essid(const char *essid, int essid_len)
 	return 1;
 }
 
-extern __inline int ieee80211_get_hdrlen(u16 fc)
+static __inline int ieee80211_get_hdrlen(u16 fc)
 {
 	int hdrlen = 24;
 
diff --git a/drivers/net/wireless/rtl8723as/include/ieee80211.h b/drivers/net/wireless/rtl8723as/include/ieee80211.h
index bf24c3b..f8046ee 100644
--- a/drivers/net/wireless/rtl8723as/include/ieee80211.h
+++ b/drivers/net/wireless/rtl8723as/include/ieee80211.h
@@ -1176,12 +1176,12 @@ enum ieee80211_state {
 (((Addr[2]) & 0xff) == 0xff) && (((Addr[3]) & 0xff) == 0xff) && (((Addr[4]) & 0xff) == 0xff) && \
 (((Addr[5]) & 0xff) == 0xff))
 #else
-extern __inline int is_multicast_mac_addr(const u8 *addr)
+static __inline int is_multicast_mac_addr(const u8 *addr)
 {
         return ((addr[0] != 0xff) && (0x01 & addr[0]));
 }
 
-extern __inline int is_broadcast_mac_addr(const u8 *addr)
+static __inline int is_broadcast_mac_addr(const u8 *addr)
 {
 	return ((addr[0] == 0xff) && (addr[1] == 0xff) && (addr[2] == 0xff) &&   \
 		(addr[3] == 0xff) && (addr[4] == 0xff) && (addr[5] == 0xff));
diff --git a/drivers/staging/rtl8712/ieee80211.h b/drivers/staging/rtl8712/ieee80211.h
index 3c0092b..1e7b55b 100644
--- a/drivers/staging/rtl8712/ieee80211.h
+++ b/drivers/staging/rtl8712/ieee80211.h
@@ -734,7 +734,7 @@ enum ieee80211_state {
 #define IEEE_G            (1<<2)
 #define IEEE_MODE_MASK    (IEEE_A|IEEE_B|IEEE_G)
 
-extern inline int ieee80211_is_empty_essid(const char *essid, int essid_len)
+static inline int ieee80211_is_empty_essid(const char *essid, int essid_len)
 {
 	/* Single white space is for Linksys APs */
 	if (essid_len == 1 && essid[0] == ' ')
@@ -748,7 +748,7 @@ extern inline int ieee80211_is_empty_essid(const char *essid, int essid_len)
 	return 1;
 }
 
-extern inline int ieee80211_get_hdrlen(u16 fc)
+static inline int ieee80211_get_hdrlen(u16 fc)
 {
 	int hdrlen = 24;
 
-- 
2.6.0.rc3

