# Optional patch for 3 lts that deactivates external 32Khz crystals and fallback to internal clock
# This fix rtc problems at the cost of clock accuracy on faulty boards
patch fix-orange-pi-3lts-rtc-on-faulty-boards.patch
