From 791849a059cce08f238491b8cae1c3d452edcda5 Mon Sep 17 00:00:00 2001
From: OpenEmbedded <oe.patch@oe>
Date: Wed, 6 Dec 2023 00:37:25 +0100
Subject: [PATCH 1/2] fix orange pi 3lts rtc on faulty boards"

---
 arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3-lts.dts | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3-lts.dts b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3-lts.dts
index 67f38b8a1..e3337c6f2 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3-lts.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-3-lts.dts
@@ -331,10 +331,10 @@ &pwm {
 &r_ir {
 	status = "okay";
 };
-
+/*
 &rtc {
 	clocks = <&ext_osc32k>;
-};
+};*/
 
 /delete-node/ &spi0;
 
-- 
2.43.0

