From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Kali Prasad <kprasadvnsi@protonmail.com>
Date: Sun, 19 Sep 2021 08:02:27 +0000
Subject: arm64: dts: allwinner: h616: Add thermal sensor and thermal zones

There are four sensors, CPU, GPU, VE, and DDR.

Signed-off-by: Kali Prasad <kprasadvnsi@protonmail.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi | 75 ++++++++++
 1 file changed, 75 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
index 7ad1982fb47f..8628a9e3dfca 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
@@ -9,6 +9,7 @@
 #include <dt-bindings/clock/sun6i-rtc.h>
 #include <dt-bindings/reset/sun50i-h616-ccu.h>
 #include <dt-bindings/reset/sun50i-h6-r-ccu.h>
+#include <dt-bindings/thermal/thermal.h>
 
 / {
 	interrupt-parent = <&gic>;
@@ -25,6 +26,8 @@ cpu0: cpu@0 {
 			reg = <0>;
 			enable-method = "psci";
 			clocks = <&ccu CLK_CPUX>;
+			clock-latency-ns = <244144>; /* 8 32k periods */
+			#cooling-cells = <2>;
 		};
 
 		cpu1: cpu@1 {
@@ -33,6 +36,8 @@ cpu1: cpu@1 {
 			reg = <1>;
 			enable-method = "psci";
 			clocks = <&ccu CLK_CPUX>;
+			clock-latency-ns = <244144>; /* 8 32k periods */
+			#cooling-cells = <2>;
 		};
 
 		cpu2: cpu@2 {
@@ -41,6 +46,8 @@ cpu2: cpu@2 {
 			reg = <2>;
 			enable-method = "psci";
 			clocks = <&ccu CLK_CPUX>;
+			clock-latency-ns = <244144>; /* 8 32k periods */
+			#cooling-cells = <2>;
 		};
 
 		cpu3: cpu@3 {
@@ -49,6 +56,8 @@ cpu3: cpu@3 {
 			reg = <3>;
 			enable-method = "psci";
 			clocks = <&ccu CLK_CPUX>;
+			clock-latency-ns = <244144>; /* 8 32k periods */
+			#cooling-cells = <2>;
 		};
 	};
 
@@ -833,5 +842,71 @@ r_rsb: rsb@7083000 {
 			#address-cells = <1>;
 			#size-cells = <0>;
 		};
+
+		ths: thermal-sensor@5070400 {
+			compatible = "allwinner,sun50i-h616-ths";
+			reg = <0x05070400 0x400>;
+			interrupts = <GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_THS>;
+			clock-names = "bus";
+			resets = <&ccu RST_BUS_THS>;
+			nvmem-cells = <&ths_calibration>;
+			nvmem-cell-names = "calibration";
+			#thermal-sensor-cells = <1>;
+		};
+	};
+
+	thermal-zones {
+		cpu-thermal {
+			polling-delay-passive = <500>;
+			polling-delay = <1000>;
+			thermal-sensors = <&ths 2>;
+			sustainable-power = <1000>;
+			k_po = <20>;
+			k_pu = <40>;
+			k_i = <0>;
+
+			trips {
+				cpu_threshold: trip-point@0 {
+					temperature = <60000>;
+					type = "passive";
+					hysteresis = <0>;
+				};
+				cpu_target: trip-point@1 {
+					temperature = <70000>;
+					type = "passive";
+					hysteresis = <0>;
+				};
+			};
+
+			cooling-maps {
+				map0 {
+					trip = <&cpu_target>;
+					cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
+							 <&cpu3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
+				};
+			};
+		};
+
+		gpu-thermal {
+			polling-delay-passive = <500>;
+			polling-delay = <1000>;
+			thermal-sensors = <&ths 0>;
+			sustainable-power = <1100>;
+		};
+
+		ve-thermal {
+			polling-delay-passive = <0>;
+			polling-delay = <0>;
+			thermal-sensors = <&ths 1>;
+		};
+
+		ddr-thermal {
+			polling-delay-passive = <0>;
+			polling-delay = <0>;
+			thermal-sensors = <&ths 3>;
+		};
 	};
 };
-- 
Armbian

