From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Jernej Skrabec <jernej.skrabec@gmail.com>
Date: Fri, 15 Oct 2021 21:14:55 +0200
Subject: arm64:dts:allwinner: sun50i-h616 Add VPU node

Signed-off-by: Jernej Skrabec <jernej.skrabec@gmail.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi | 24 ++++++++++
 1 file changed, 24 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
index 26ef79c5d895..944ff2747d27 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
@@ -122,6 +122,17 @@ gpu: gpu@1800000 {
 			status = "disabled";
 		};
 
+		video-codec@1c0e000 {
+			compatible = "allwinner,sun50i-h616-video-engine";
+			reg = <0x01c0e000 0x2000>;
+			clocks = <&ccu CLK_BUS_VE>, <&ccu CLK_VE>,
+				 <&ccu CLK_MBUS_VE>;
+			clock-names = "ahb", "mod", "ram";
+			resets = <&ccu RST_BUS_VE>;
+			interrupts = <GIC_SPI 93 IRQ_TYPE_LEVEL_HIGH>;
+			allwinner,sram = <&ve_sram 1>;
+		};
+
 		syscon: syscon@3000000 {
 			compatible = "allwinner,sun50i-h616-system-control";
 			reg = <0x03000000 0x1000>;
@@ -136,6 +147,19 @@ sram_c: sram@28000 {
 				#size-cells = <1>;
 				ranges = <0 0x00028000 0x30000>;
 			};
+
+			sram_c1: sram@1a00000 {
+				compatible = "mmio-sram";
+				reg = <0x01a00000 0x200000>;
+				#address-cells = <1>;
+				#size-cells = <1>;
+				ranges = <0 0x01a00000 0x200000>;
+
+				ve_sram: sram-section@0 {
+					compatible = "allwinner,sun50i-h616-sram-c1";
+					reg = <0x000000 0x200000>;
+				};
+			};
 		};
 
 		ccu: clock@3001000 {
-- 
Armbian

