IMAGE_BOOT_FILES:append:orange-pi-zero2w = " boot.scr ${KERNEL_DEVICETREE} diya-config.txt recovery-${MACHINE}.cpio.lz4.u-boot Image.gz "
# ${KERNEL_DEVICETREE} allwinner/overlay/sun50i-h616-fixup.scr "
IMAGE_INSTALL:append:orange-pi-zero2w = " uwe5622-firmware diya-resizefs "
OVERLAYFS_ETC_DEVICE = "/dev/mmcblk0p3"