IMAGE_BOOT_FILES:append:pinephone = " boot.scr ${KERNEL_DEVICETREE} diya-config.txt recovery-${MACHINE}.cpio.lz4.u-boot Image.gz "
OVERLAYFS_ETC_DEVICE = "/dev/mmcblk0p3"
IMAGE_INSTALL:append:pinephone = " \
    pinephone-firmware \
    eg25-manager \
    modemmanager \
    gpsd \
    gps-utils \
    diya-resizefs \
    "