From f487f62babb11d014da7a0b58a0fcdf6d217a812 Mon Sep 17 00:00:00 2001
From: Marek Belisko <marek.belisko@open-nandra.com>
Date: Thu, 11 May 2023 11:18:33 +0200
Subject: [PATCH] bananapi-m64: Consistent nodes for mmc devices

Signed-off-by: Marek Belisko <marek.belisko@open-nandra.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-a64-bananapi-m64.dts | 3 +++
 1 file changed, 3 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-bananapi-m64.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-bananapi-m64.dts
index e6d5bc0f7..39a28aad8 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-bananapi-m64.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-bananapi-m64.dts
@@ -16,6 +16,9 @@ aliases {
 		ethernet0 = &emac;
 		serial0 = &uart0;
 		serial1 = &uart1;
+                mmc0 = &mmc0;
+                mmc1 = &mmc1;
+                mmc2 = &mmc2;
 	};
 
 	chosen {
-- 
2.25.1

