From 0000000000000000000000000000000000000000 Mon Sep 17 00:00:00 2001
From: Jernej Skrabec <jernej.skrabec@gmail.com>
Date: Fri, 15 Oct 2021 21:07:46 +0200
Subject: arm64:dts: allwinner: sun50i-h616 Add GPU node

Signed-off-by: Jernej Skrabec <jernej.skrabec@gmail.com>
---
 arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi | 14 ++++++++++
 1 file changed, 14 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
index 44f8ae11ca16..26ef79c5d895 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616.dtsi
@@ -108,6 +108,20 @@ soc {
 		#size-cells = <1>;
 		ranges = <0x0 0x0 0x0 0x40000000>;
 
+		gpu: gpu@1800000 {
+			compatible = "allwinner,sun50i-h616-mali",
+				     "arm,mali-bifrost";
+			reg = <0x1800000 0x40000>;
+			interrupts = <GIC_SPI 95 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "job", "mmu", "gpu";
+			clocks = <&ccu CLK_GPU0>, <&ccu CLK_BUS_GPU>;
+			clock-names = "core", "bus";
+			resets = <&ccu RST_BUS_GPU>;
+			status = "disabled";
+		};
+
 		syscon: syscon@3000000 {
 			compatible = "allwinner,sun50i-h616-system-control";
 			reg = <0x03000000 0x1000>;
-- 
Armbian

