From bf813915bf480154c707e0be14016cef94adbd95 Mon Sep 17 00:00:00 2001
From: Marek Belisko <marek.belisko@gmail.com>
Date: Tue, 7 May 2024 11:27:08 +0200
Subject: [PATCH] mangopi-mq-r-t113: Fix serial console

Serial console is on uart3 not on uart0.

Upstream-Status: Inappropriate (for this board only)

Signed-off-by: Marek Belisko <marek.belisko@gmail.com>
---
 include/configs/sunxi-common.h | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

diff --git a/include/configs/sunxi-common.h b/include/configs/sunxi-common.h
index b8ca77d031..4e4808d2c1 100644
--- a/include/configs/sunxi-common.h
+++ b/include/configs/sunxi-common.h
@@ -324,7 +324,7 @@
 	MEM_LAYOUT_ENV_EXTRA_SETTINGS \
 	DFU_ALT_INFO_RAM \
 	"fdtfile=" FDTFILE "\0" \
-	"console=ttyS0,115200\0" \
+	"console=ttyS3,115200\0" \
 	"uuid_gpt_esp=" UUID_GPT_ESP "\0" \
 	"uuid_gpt_system=" UUID_GPT_SYSTEM "\0" \
 	"partitions=" PARTS_DEFAULT "\0" \
-- 
2.25.1

