From 6a64d90ca4d976c16a2e102dbad0848e4d29776c Mon Sep 17 00:00:00 2001
From: Florin Sarbu <florin@resin.io>
Date: Wed, 12 Sep 2018 14:22:49 +0200
Subject: [PATCH] nanopi_neo_air_defconfig: Enable eMMC support

Upstream-Status: Pending
Signed-off-by: Florin Sarbu <florin@resin.io>

---
 configs/nanopi_neo_air_defconfig | 1 +
 1 file changed, 1 insertion(+)

diff --git a/configs/nanopi_neo_air_defconfig b/configs/nanopi_neo_air_defconfig
index 806d95c1cc..8899cc3a15 100644
--- a/configs/nanopi_neo_air_defconfig
+++ b/configs/nanopi_neo_air_defconfig
@@ -9,3 +9,4 @@ CONFIG_DRAM_CLK=408
 CONFIG_CONSOLE_MUX=y
 CONFIG_USB_EHCI_HCD=y
 CONFIG_USB_OHCI_HCD=y
+CONFIG_MMC_SUNXI_SLOT_EXTRA=2
