From 7d7f32460702e99cab48909bb85ed84b67e65062 Mon Sep 17 00:00:00 2001
From: Marek Belisko <marek.belisko@open-nandra.com>
Date: Tue, 24 Oct 2023 10:43:55 +0200
Subject: [PATCH] dts: allwinner: bananapi-m2-zero: Enforce consistent MMC
 numbering

Enforce MMC number (sometimes the order was wrong and the device does not boot).

Upstream-Status: Pending

Signed-off-by: Marek Belisko <marek.belisko@open-nandra.com>
---
 arch/arm/boot/dts/allwinner/sun8i-h2-plus-bananapi-m2-zero.dts | 3 +++
 1 file changed, 3 insertions(+)

diff --git a/arch/arm/boot/dts/allwinner/sun8i-h2-plus-bananapi-m2-zero.dts b/arch/arm/boot/dts/allwinner/sun8i-h2-plus-bananapi-m2-zero.dts
index d729b7c70..410a79487 100644
--- a/arch/arm/boot/dts/allwinner/sun8i-h2-plus-bananapi-m2-zero.dts
+++ b/arch/arm/boot/dts/allwinner/sun8i-h2-plus-bananapi-m2-zero.dts
@@ -20,6 +20,9 @@ / {
 	aliases {
 		serial0 = &uart0;
 		serial1 = &uart1;
+		mmc0 = &mmc0;
+		mmc1 = &mmc1;
+		mmc2 = &mmc2;
 	};
 
 	chosen {
-- 
2.25.1

