From: Dany LE <dany@iohub.dev>
Date: Wed, 8 Apr 2025 20:16:14 -0800
Subject: enable mali GPU

Upstream-Status: Pending

---
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero2w.dts b/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero2w.dts
index 27e817b379a4..01d2d6682c67 100755
--- a/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero2w.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h616-orangepi-zero2w.dts
@@ -134,7 +134,7 @@ hdmi_out_con: endpoint {
 
 &gpu {
 	mali-supply = <&reg_dcdc1>;
-	status = "disabled";
+	status = "okay";
 };
 
 &mmc0 {
